gif2bgi

Go to index page.

# gif2epsn

A program to dump images saved as GIF files on Epson type printers.

# Usage:

    gif2epsn [-q] [-d dither] [-t bw] [-m map] [-i] [-n] [-p printer] [-h] gif-file

If no gif-file is given, Gif2Epsn will try to read a GIF file from stdin.

# Memory required:

Screen.

# Options:

[-q]
  Quiet mode. Default off on MSDOS, on under UNIX. Controls printout of running scan lines. Use -q- to invert.

[-d dither]
  Sets size of dithering matrix, where DitherSize can be 2,3 or 4 only (for 2x2, 3x3 and 4x4 dithering matrices). Default is 2. Note image will be displayed in this mode only if the mapping option (see -m) selected this mode.

[-t bw]
  Sets threshold level for B&W mapping in percent. This threshold level is used in the different mappings as selected via -m. Default is 19%.

[-m map]
  Select method to map colors to B&W. Mapping can be:
  0
    Every none background color is considered foreground (white color but is drawn as black by printer, unless -i is specified).

  1
    If 0.3 * RED + 0.59 * GREEN + 0.11 * YELLOW > BW the pixel is considered white color.

  2
    Colors are mapped as in 1, and use dithering of size as defined using -d option. BWthreshold is used here as scaler.

  The default is option 0.

[-i]
  Invert the image, i.e. black -> white, white -> black.

[-n]
  Nicer image. Uses double-density feature of Epson printer. This takes more time (and kills your ink cartridge faster...) but results are usually better.

[-p printer]
  Under Unix, output goes to stdout by default; under DOS, the default is LPT1:. With this switch you can specify the output target.

[-h]
  print one line of command line help, similar to Usage above.

# Notes:

The output has an aspect ratio of 1, so a square image will be square in hardcopy as well.

The widest image can be printed is 640 pixels, on 8 inch paper. You probably will need to flip wider images, if height is less than that: `gifflip -r x29.gif | gif2epsn'. Wider images will be clipped.

# Author:

Gershon Elber