Manpage of TIFF2BW

# TIFF2BW

Section: User Commands (1)
Updated: October 15, 1995
Index
Return to Main Contents

## NAME

tiff2bw - convert a color TIFF image to greyscale

## SYNOPSIS

tiff2bw [ options ] input.tif output.tif

## DESCRIPTION

Tiff2bw converts an RGB or Palette color TIFF image to a greyscale image by combining percentages of the red, green, and blue channels. By default, output samples are created by taking 28% of the red channel, 59% of the green channel, and 11% of the blue channel. To alter these percentages, the -R, -G, and -B options may be used.

## OPTIONS

-c
  Specify a compression scheme to use when writing image data: -c none for no compression, -c packbits for the PackBits compression algorithm, -c zip for the Deflate compression algorithm, -c g3 for the CCITT Group 3 compression algorithm, -c g4 for the CCITT Group 4 compression algorithm, and -c lzw for Lempel-Ziv & Welch (the default).
-r
  Write data with a specified number of rows per strip; by default the number of rows/strip is selected so that each strip is approximately 8 kilobytes.
-R
  Specify the percentage of the red channel to use (default 28).
-G
  Specify the percentage of the green channel to use (default 59).
-B
  Specify the percentage of the blue channel to use (default 11).

## SEE ALSO

pal2rgb(1), tiffinfo(1), tiffcp(1), tiffmedian(1), libtiff(3)

## Index

NAME
SYNOPSIS
DESCRIPTION
OPTIONS
SEE ALSO

This document was created by man2html, using the manual pages.
Time: 01:31:47 GMT, November 23, 1999